1. Install Arduino IDE

2. Get USB to UART driver https://www.silabs.com/products/development-tools/software/usb-to-uart-bridge-vcp-drivers

3. Add ESP1266 Board Manager -

https://github.com/esp8266/Arduino

http://arduino.esp8266.com/stable/package\_esp8266com\_index.json

4. Select the "Generic ESP8666 Module"

5. Open ""

5. https://arduino-esp8266.readthedocs.io/en/latest/

Other Links

ESP8266 User guide - https://tttapa.github.io/ESP8266/Chap01%20-%20ESP8266.html

<https://www.instructables.com/id/A-Beginners-Guide-to-Arduino/>









